(kicad_symbol_lib
  (version 20211014)
  (generator FastEDA)
  (symbol "TYPE-C-31-M-12"
    (in_bom yes)
    (on_board yes)
    (property
      "Reference"
      "USBC"
      (id 0)
      (at 0 19.05 0)
    )
    (property
      "Value"
      "TYPE-C-31-M-12"
      (id 1)
      (at 0 -19.05 0)
    )
    (property
      "Footprint"
      "C165948:USB-C_SMD-TYPE-C-31-M-12_1"
      (id 2)
      (at 0 -21.59 0)
    )
    (property
      "Datasheet"
      "https://lcsc.com/product-detail/USB-Type-C_Korean-Hroparts-Elec-TYPE-C-31-M-12_C165948.html"
      (id 3)
      (at 0 -24.13 0)
    )
    (property
      "Manufacturer"
      "韩国韩荣"
      (id 4)
      (at 0 -26.67 0)
    )
    (property
      "MPN"
      "TYPE-C-31-M-12"
      (id 5)
      (at 0 -29.21 0)
    )
    (property
      "LCSC Part"
      "C165948"
      (id 6)
      (at 0 -31.75 0)
    )
    (property
      "ki_keywords"
      "USB Connectors"
      (id 8)
      (at 0 -34.29 0)
    )
    (symbol "TYPE-C-31-M-12_0_1"
      (pin unspecified line
        (at -6.35 13.97 0)
        (length 2.54)
        (name "GND")
        (number "A1B12")
      )
      (pin unspecified line
        (at -6.35 11.43 0)
        (length 2.54)
        (name "VBUS")
        (number "A4B9")
      )
      (pin unspecified line
        (at -6.35 8.89 0)
        (length 2.54)
        (name "SBU2")
        (number "B8")
      )
      (pin unspecified line
        (at -6.35 6.35 0)
        (length 2.54)
        (name "CC1")
        (number "A5")
      )
      (pin unspecified line
        (at -6.35 3.81 0)
        (length 2.54)
        (name "DN2")
        (number "B7")
      )
      (pin unspecified line
        (at -6.35 1.27 0)
        (length 2.54)
        (name "DP1")
        (number "A6")
      )
      (pin unspecified line
        (at -6.35 -1.27 0)
        (length 2.54)
        (name "DN1")
        (number "A7")
      )
      (pin unspecified line
        (at -6.35 -3.81 0)
        (length 2.54)
        (name "DP2")
        (number "B6")
      )
      (pin unspecified line
        (at -6.35 -6.35 0)
        (length 2.54)
        (name "SBU1")
        (number "A8")
      )
      (pin unspecified line
        (at -6.35 -8.89 0)
        (length 2.54)
        (name "CC2")
        (number "B5")
      )
      (pin unspecified line
        (at -6.35 -11.43 0)
        (length 2.54)
        (name "VBUS")
        (number "B4A9")
      )
      (pin unspecified line
        (at -6.35 -13.97 0)
        (length 2.54)
        (name "GND")
        (number "B1A12")
      )
      (pin unspecified line
        (at 11.43 -6.35 180)
        (length 2.54)
        (name "EH")
        (number "4")
      )
      (pin unspecified line
        (at 11.43 -8.89 180)
        (length 2.54)
        (name "EH")
        (number "3")
      )
      (pin unspecified line
        (at 11.43 -11.43 180)
        (length 2.54)
        (name "EH")
        (number "2")
      )
      (pin unspecified line
        (at 11.43 -13.97 180)
        (length 2.54)
        (name "EH")
        (number "1")
      )
    )
  )
)