(kicad_symbol_lib
  (version 20211014)
  (generator FastEDA)
  (symbol "ESP32-PICO-D4"
    (in_bom yes)
    (on_board yes)
    (property
      "Reference"
      "U"
      (id 0)
      (at 0 35.56 0)
    )
    (property
      "Value"
      "ESP32-PICO-D4"
      (id 1)
      (at 0 -35.56 0)
    )
    (property
      "Footprint"
      "C193707:LGA-48_L7.0-W7.0-P0.50-BL-EP5.4"
      (id 2)
      (at 0 -38.10 0)
    )
    (property
      "Datasheet"
      "https://lcsc.com/product-detail/Others_Espressif-Systems-ESP32-PICO-D4_C193707.html"
      (id 3)
      (at 0 -40.64 0)
    )
    (property
      "Manufacturer"
      "ESPRESSIF(乐鑫)"
      (id 4)
      (at 0 -43.18 0)
    )
    (property
      "MPN"
      "ESP32-PICO-D4"
      (id 5)
      (at 0 -45.72 0)
    )
    (property
      "LCSC Part"
      "C193707"
      (id 6)
      (at 0 -48.26 0)
    )
    (property
      "ki_keywords"
      "RF Transceiver ICs"
      (id 8)
      (at 0 -50.80 0)
    )
    (symbol "ESP32-PICO-D4_0_1"
      (pin unspecified line
        (at -22.86 27.94 0)
        (length 2.54)
        (name "VDDA")
        (number "1")
      )
      (pin unspecified line
        (at -22.86 25.40 0)
        (length 2.54)
        (name "LNA_IN")
        (number "2")
      )
      (pin unspecified line
        (at -22.86 22.86 0)
        (length 2.54)
        (name "VDDA3P3")
        (number "3")
      )
      (pin unspecified line
        (at -22.86 20.32 0)
        (length 2.54)
        (name "VDDA3P3")
        (number "4")
      )
      (pin unspecified line
        (at -22.86 17.78 0)
        (length 2.54)
        (name "SENSOR_VP")
        (number "5")
      )
      (pin unspecified line
        (at -22.86 15.24 0)
        (length 2.54)
        (name "SENSOR_CAPP")
        (number "6")
      )
      (pin unspecified line
        (at -22.86 12.70 0)
        (length 2.54)
        (name "SENSOR_CAPN")
        (number "7")
      )
      (pin unspecified line
        (at -22.86 10.16 0)
        (length 2.54)
        (name "SENSOR_VN")
        (number "8")
      )
      (pin unspecified line
        (at -22.86 7.62 0)
        (length 2.54)
        (name "EN")
        (number "9")
      )
      (pin unspecified line
        (at -22.86 5.08 0)
        (length 2.54)
        (name "IO34")
        (number "10")
      )
      (pin unspecified line
        (at -22.86 2.54 0)
        (length 2.54)
        (name "IO35")
        (number "11")
      )
      (pin unspecified line
        (at -22.86 -0.00 0)
        (length 2.54)
        (name "IO32")
        (number "12")
      )
      (pin unspecified line
        (at -22.86 -2.54 0)
        (length 2.54)
        (name "IO33")
        (number "13")
      )
      (pin unspecified line
        (at -22.86 -5.08 0)
        (length 2.54)
        (name "IO25")
        (number "14")
      )
      (pin unspecified line
        (at -22.86 -7.62 0)
        (length 2.54)
        (name "IO26")
        (number "15")
      )
      (pin unspecified line
        (at -22.86 -10.16 0)
        (length 2.54)
        (name "IO27")
        (number "16")
      )
      (pin unspecified line
        (at -22.86 -12.70 0)
        (length 2.54)
        (name "IO14")
        (number "17")
      )
      (pin unspecified line
        (at -22.86 -15.24 0)
        (length 2.54)
        (name "IO12")
        (number "18")
      )
      (pin unspecified line
        (at -22.86 -17.78 0)
        (length 2.54)
        (name "VDD3P3_RTC")
        (number "19")
      )
      (pin unspecified line
        (at -22.86 -20.32 0)
        (length 2.54)
        (name "IO13")
        (number "20")
      )
      (pin unspecified line
        (at -22.86 -22.86 0)
        (length 2.54)
        (name "IO15")
        (number "21")
      )
      (pin unspecified line
        (at -22.86 -25.40 0)
        (length 2.54)
        (name "IO2")
        (number "22")
      )
      (pin unspecified line
        (at -22.86 -27.94 0)
        (length 2.54)
        (name "IO0")
        (number "23")
      )
      (pin unspecified line
        (at -22.86 -30.48 0)
        (length 2.54)
        (name "IO4")
        (number "24")
      )
      (pin unspecified line
        (at 22.86 -30.48 180)
        (length 2.54)
        (name "IO16")
        (number "25")
      )
      (pin unspecified line
        (at 22.86 -27.94 180)
        (length 2.54)
        (name "VDD_SDIO")
        (number "26")
      )
      (pin unspecified line
        (at 22.86 -25.40 180)
        (length 2.54)
        (name "IO17")
        (number "27")
      )
      (pin unspecified line
        (at 22.86 -22.86 180)
        (length 2.54)
        (name "SD2")
        (number "28")
      )
      (pin unspecified line
        (at 22.86 -20.32 180)
        (length 2.54)
        (name "SD3")
        (number "29")
      )
      (pin unspecified line
        (at 22.86 -17.78 180)
        (length 2.54)
        (name "CMD")
        (number "30")
      )
      (pin unspecified line
        (at 22.86 -15.24 180)
        (length 2.54)
        (name "CLK")
        (number "31")
      )
      (pin unspecified line
        (at 22.86 -12.70 180)
        (length 2.54)
        (name "SD0")
        (number "32")
      )
      (pin unspecified line
        (at 22.86 -10.16 180)
        (length 2.54)
        (name "SD1")
        (number "33")
      )
      (pin unspecified line
        (at 22.86 -7.62 180)
        (length 2.54)
        (name "IO5")
        (number "34")
      )
      (pin unspecified line
        (at 22.86 -5.08 180)
        (length 2.54)
        (name "IO18")
        (number "35")
      )
      (pin unspecified line
        (at 22.86 -2.54 180)
        (length 2.54)
        (name "IO23")
        (number "36")
      )
      (pin unspecified line
        (at 22.86 -0.00 180)
        (length 2.54)
        (name "VDD3P3_CPU")
        (number "37")
      )
      (pin unspecified line
        (at 22.86 2.54 180)
        (length 2.54)
        (name "IO19")
        (number "38")
      )
      (pin unspecified line
        (at 22.86 5.08 180)
        (length 2.54)
        (name "IO22")
        (number "39")
      )
      (pin unspecified line
        (at 22.86 7.62 180)
        (length 2.54)
        (name "U0RXD")
        (number "40")
      )
      (pin unspecified line
        (at 22.86 10.16 180)
        (length 2.54)
        (name "U0TXD")
        (number "41")
      )
      (pin unspecified line
        (at 22.86 12.70 180)
        (length 2.54)
        (name "IO21")
        (number "42")
      )
      (pin unspecified line
        (at 22.86 15.24 180)
        (length 2.54)
        (name "VDDA")
        (number "43")
      )
      (pin unspecified line
        (at 22.86 17.78 180)
        (length 2.54)
        (name "XTAL_N_NC")
        (number "44")
      )
      (pin unspecified line
        (at 22.86 20.32 180)
        (length 2.54)
        (name "XTAL_P_NC")
        (number "45")
      )
      (pin unspecified line
        (at 22.86 22.86 180)
        (length 2.54)
        (name "VDDA")
        (number "46")
      )
      (pin unspecified line
        (at 22.86 25.40 180)
        (length 2.54)
        (name "CAP2_NC")
        (number "47")
      )
      (pin unspecified line
        (at 22.86 27.94 180)
        (length 2.54)
        (name "CAP1_NC")
        (number "48")
      )
      (pin unspecified line
        (at 22.86 30.48 180)
        (length 2.54)
        (name "GND")
        (number "49")
      )
    )
  )
)