(kicad_symbol_lib
  (version 20211014)
  (generator FastEDA)
  (symbol "ESP32-C3-MINI-1-N4"
    (in_bom yes)
    (on_board yes)
    (property
      "Reference"
      "U"
      (id 0)
      (at 0 38.10 0)
    )
    (property
      "Value"
      "ESP32-C3-MINI-1-N4"
      (id 1)
      (at 0 -38.10 0)
    )
    (property
      "Footprint"
      "C2838502:WIFIM-SMD_ESP32-C3-MINI-1"
      (id 2)
      (at 0 -40.64 0)
    )
    (property
      "Datasheet"
      "https://www.lcsc.com/datasheet/C2838502.pdf"
      (id 3)
      (at 0 -43.18 0)
    )
    (property
      "Manufacturer"
      "ESPRESSIF(乐鑫)"
      (id 4)
      (at 0 -45.72 0)
    )
    (property
      "MPN"
      "ESP32-C3-MINI-1-N4"
      (id 5)
      (at 0 -48.26 0)
    )
    (property
      "LCSC Part"
      "C2838502"
      (id 6)
      (at 0 -50.80 0)
    )
    (property
      "ki_keywords"
      "Wireless Modules"
      (id 8)
      (at 0 -53.34 0)
    )
    (symbol "ESP32-C3-MINI-1-N4_0_1"
      (pin unspecified line
        (at -11.43 30.48 0)
        (length 2.54)
        (name "GND")
        (number "1")
      )
      (pin unspecified line
        (at -11.43 27.94 0)
        (length 2.54)
        (name "GND")
        (number "2")
      )
      (pin unspecified line
        (at -11.43 25.40 0)
        (length 2.54)
        (name "3V3")
        (number "3")
      )
      (pin unspecified line
        (at -11.43 22.86 0)
        (length 2.54)
        (name "NC")
        (number "4")
      )
      (pin unspecified line
        (at -11.43 20.32 0)
        (length 2.54)
        (name "IO2")
        (number "5")
      )
      (pin unspecified line
        (at -11.43 17.78 0)
        (length 2.54)
        (name "IO3")
        (number "6")
      )
      (pin unspecified line
        (at -11.43 15.24 0)
        (length 2.54)
        (name "NC")
        (number "7")
      )
      (pin unspecified line
        (at -11.43 12.70 0)
        (length 2.54)
        (name "EN")
        (number "8")
      )
      (pin unspecified line
        (at -11.43 10.16 0)
        (length 2.54)
        (name "NC")
        (number "9")
      )
      (pin unspecified line
        (at -11.43 7.62 0)
        (length 2.54)
        (name "NC")
        (number "10")
      )
      (pin unspecified line
        (at -11.43 5.08 0)
        (length 2.54)
        (name "GND")
        (number "11")
      )
      (pin unspecified line
        (at -11.43 2.54 0)
        (length 2.54)
        (name "IO0")
        (number "12")
      )
      (pin unspecified line
        (at -11.43 -0.00 0)
        (length 2.54)
        (name "IO1")
        (number "13")
      )
      (pin unspecified line
        (at -11.43 -2.54 0)
        (length 2.54)
        (name "GND")
        (number "14")
      )
      (pin unspecified line
        (at -11.43 -5.08 0)
        (length 2.54)
        (name "NC")
        (number "15")
      )
      (pin unspecified line
        (at -11.43 -7.62 0)
        (length 2.54)
        (name "IO10")
        (number "16")
      )
      (pin unspecified line
        (at -11.43 -10.16 0)
        (length 2.54)
        (name "NC")
        (number "17")
      )
      (pin unspecified line
        (at -11.43 -12.70 0)
        (length 2.54)
        (name "IO4")
        (number "18")
      )
      (pin unspecified line
        (at -11.43 -15.24 0)
        (length 2.54)
        (name "IO5")
        (number "19")
      )
      (pin unspecified line
        (at -11.43 -17.78 0)
        (length 2.54)
        (name "IO6")
        (number "20")
      )
      (pin unspecified line
        (at -11.43 -20.32 0)
        (length 2.54)
        (name "IO7")
        (number "21")
      )
      (pin unspecified line
        (at -11.43 -22.86 0)
        (length 2.54)
        (name "IO8")
        (number "22")
      )
      (pin unspecified line
        (at -11.43 -25.40 0)
        (length 2.54)
        (name "IO9")
        (number "23")
      )
      (pin unspecified line
        (at -11.43 -27.94 0)
        (length 2.54)
        (name "NC")
        (number "24")
      )
      (pin unspecified line
        (at -11.43 -30.48 0)
        (length 2.54)
        (name "NC")
        (number "25")
      )
      (pin unspecified line
        (at -11.43 -33.02 0)
        (length 2.54)
        (name "IO18")
        (number "26")
      )
      (pin unspecified line
        (at 11.43 -33.02 180)
        (length 2.54)
        (name "IO19")
        (number "27")
      )
      (pin unspecified line
        (at 11.43 -30.48 180)
        (length 2.54)
        (name "NC")
        (number "28")
      )
      (pin unspecified line
        (at 11.43 -27.94 180)
        (length 2.54)
        (name "NC")
        (number "29")
      )
      (pin unspecified line
        (at 11.43 -25.40 180)
        (length 2.54)
        (name "RXD0")
        (number "30")
      )
      (pin unspecified line
        (at 11.43 -22.86 180)
        (length 2.54)
        (name "TXD0")
        (number "31")
      )
      (pin unspecified line
        (at 11.43 -20.32 180)
        (length 2.54)
        (name "NC")
        (number "32")
      )
      (pin unspecified line
        (at 11.43 -17.78 180)
        (length 2.54)
        (name "NC")
        (number "33")
      )
      (pin unspecified line
        (at 11.43 -15.24 180)
        (length 2.54)
        (name "NC")
        (number "34")
      )
      (pin unspecified line
        (at 11.43 -12.70 180)
        (length 2.54)
        (name "NC")
        (number "35")
      )
      (pin unspecified line
        (at 11.43 -10.16 180)
        (length 2.54)
        (name "GND")
        (number "36")
      )
      (pin unspecified line
        (at 11.43 -7.62 180)
        (length 2.54)
        (name "GND")
        (number "37")
      )
      (pin unspecified line
        (at 11.43 -5.08 180)
        (length 2.54)
        (name "GND")
        (number "38")
      )
      (pin unspecified line
        (at 11.43 -2.54 180)
        (length 2.54)
        (name "GND")
        (number "39")
      )
      (pin unspecified line
        (at 11.43 -0.00 180)
        (length 2.54)
        (name "GND")
        (number "40")
      )
      (pin unspecified line
        (at 11.43 2.54 180)
        (length 2.54)
        (name "GND")
        (number "41")
      )
      (pin unspecified line
        (at 11.43 5.08 180)
        (length 2.54)
        (name "GND")
        (number "42")
      )
      (pin unspecified line
        (at 11.43 7.62 180)
        (length 2.54)
        (name "GND")
        (number "43")
      )
      (pin unspecified line
        (at 11.43 10.16 180)
        (length 2.54)
        (name "GND")
        (number "44")
      )
      (pin unspecified line
        (at 11.43 12.70 180)
        (length 2.54)
        (name "GND")
        (number "45")
      )
      (pin unspecified line
        (at 11.43 15.24 180)
        (length 2.54)
        (name "GND")
        (number "46")
      )
      (pin unspecified line
        (at 11.43 17.78 180)
        (length 2.54)
        (name "GND")
        (number "47")
      )
      (pin unspecified line
        (at 11.43 20.32 180)
        (length 2.54)
        (name "GND")
        (number "48")
      )
      (pin unspecified line
        (at 11.43 22.86 180)
        (length 2.54)
        (name "GND")
        (number "49")
      )
      (pin unspecified line
        (at 11.43 25.40 180)
        (length 2.54)
        (name "GND")
        (number "50")
      )
      (pin unspecified line
        (at 11.43 27.94 180)
        (length 2.54)
        (name "GND")
        (number "51")
      )
      (pin unspecified line
        (at 11.43 30.48 180)
        (length 2.54)
        (name "GND")
        (number "52")
      )
      (pin unspecified line
        (at 11.43 33.02 180)
        (length 2.54)
        (name "GND")
        (number "53")
      )
    )
  )
)