(kicad_symbol_lib
  (version 20211014)
  (generator FastEDA)
  (symbol "ESP32-S3-WROOM-1-N8"
    (in_bom yes)
    (on_board yes)
    (property
      "Reference"
      "U"
      (id 0)
      (at 0 19.05 0)
    )
    (property
      "Value"
      "ESP32-S3-WROOM-1-N8"
      (id 1)
      (at 0 -35.56 0)
    )
    (property
      "Footprint"
      "C2913198:WIFIM-SMD_ESP32-S3-WROOM-1-N8"
      (id 2)
      (at 0 -38.10 0)
    )
    (property
      "Datasheet"
      "https://www.lcsc.com/datasheet/C2913198.pdf"
      (id 3)
      (at 0 -40.64 0)
    )
    (property
      "Manufacturer"
      "ESPRESSIF(乐鑫)"
      (id 4)
      (at 0 -43.18 0)
    )
    (property
      "MPN"
      "ESP32-S3-WROOM-1-N8"
      (id 5)
      (at 0 -45.72 0)
    )
    (property
      "LCSC Part"
      "C2913198"
      (id 6)
      (at 0 -48.26 0)
    )
    (property
      "ki_keywords"
      "WiFi Modules"
      (id 8)
      (at 0 -50.80 0)
    )
    (symbol "ESP32-S3-WROOM-1-N8_0_1"
      (pin unspecified line
        (at -21.59 12.70 0)
        (length 2.54)
        (name "GND")
        (number "1")
      )
      (pin unspecified line
        (at -21.59 10.16 0)
        (length 2.54)
        (name "3V3")
        (number "2")
      )
      (pin unspecified line
        (at -21.59 7.62 0)
        (length 2.54)
        (name "EN")
        (number "3")
      )
      (pin unspecified line
        (at -21.59 5.08 0)
        (length 2.54)
        (name "IO4")
        (number "4")
      )
      (pin unspecified line
        (at -21.59 2.54 0)
        (length 2.54)
        (name "IO5")
        (number "5")
      )
      (pin unspecified line
        (at -21.59 -0.00 0)
        (length 2.54)
        (name "IO6")
        (number "6")
      )
      (pin unspecified line
        (at -21.59 -2.54 0)
        (length 2.54)
        (name "IO7")
        (number "7")
      )
      (pin unspecified line
        (at -21.59 -5.08 0)
        (length 2.54)
        (name "IO15")
        (number "8")
      )
      (pin unspecified line
        (at -21.59 -7.62 0)
        (length 2.54)
        (name "IO16")
        (number "9")
      )
      (pin unspecified line
        (at -21.59 -10.16 0)
        (length 2.54)
        (name "IO17")
        (number "10")
      )
      (pin unspecified line
        (at -21.59 -12.70 0)
        (length 2.54)
        (name "IO18")
        (number "11")
      )
      (pin unspecified line
        (at -21.59 -15.24 0)
        (length 2.54)
        (name "IO8")
        (number "12")
      )
      (pin unspecified line
        (at -21.59 -17.78 0)
        (length 2.54)
        (name "IO19")
        (number "13")
      )
      (pin unspecified line
        (at -21.59 -20.32 0)
        (length 2.54)
        (name "IO20")
        (number "14")
      )
      (pin unspecified line
        (at -12.70 -30.48 90)
        (length 2.54)
        (name "IO3")
        (number "15")
      )
      (pin unspecified line
        (at -10.16 -30.48 90)
        (length 2.54)
        (name "IO46")
        (number "16")
      )
      (pin unspecified line
        (at -7.62 -30.48 90)
        (length 2.54)
        (name "IO9")
        (number "17")
      )
      (pin unspecified line
        (at -5.08 -30.48 90)
        (length 2.54)
        (name "IO10")
        (number "18")
      )
      (pin unspecified line
        (at -2.54 -30.48 90)
        (length 2.54)
        (name "IO11")
        (number "19")
      )
      (pin unspecified line
        (at 0.00 -30.48 90)
        (length 2.54)
        (name "IO12")
        (number "20")
      )
      (pin unspecified line
        (at 2.54 -30.48 90)
        (length 2.54)
        (name "IO13")
        (number "21")
      )
      (pin unspecified line
        (at 5.08 -30.48 90)
        (length 2.54)
        (name "IO14")
        (number "22")
      )
      (pin unspecified line
        (at 7.62 -30.48 90)
        (length 2.54)
        (name "IO21")
        (number "23")
      )
      (pin unspecified line
        (at 10.16 -30.48 90)
        (length 2.54)
        (name "IO47")
        (number "24")
      )
      (pin unspecified line
        (at 12.70 -30.48 90)
        (length 2.54)
        (name "IO48")
        (number "25")
      )
      (pin unspecified line
        (at 15.24 -30.48 90)
        (length 2.54)
        (name "IO45")
        (number "26")
      )
      (pin unspecified line
        (at 22.86 -19.05 180)
        (length 2.54)
        (name "IO0")
        (number "27")
      )
      (pin unspecified line
        (at 22.86 -16.51 180)
        (length 2.54)
        (name "IO35")
        (number "28")
      )
      (pin unspecified line
        (at 22.86 -13.97 180)
        (length 2.54)
        (name "IO36")
        (number "29")
      )
      (pin unspecified line
        (at 22.86 -11.43 180)
        (length 2.54)
        (name "IO37")
        (number "30")
      )
      (pin unspecified line
        (at 22.86 -8.89 180)
        (length 2.54)
        (name "IO38")
        (number "31")
      )
      (pin unspecified line
        (at 22.86 -6.35 180)
        (length 2.54)
        (name "IO39")
        (number "32")
      )
      (pin unspecified line
        (at 22.86 -3.81 180)
        (length 2.54)
        (name "IO40")
        (number "33")
      )
      (pin unspecified line
        (at 22.86 -1.27 180)
        (length 2.54)
        (name "IO41")
        (number "34")
      )
      (pin unspecified line
        (at 22.86 1.27 180)
        (length 2.54)
        (name "IO42")
        (number "35")
      )
      (pin unspecified line
        (at 22.86 3.81 180)
        (length 2.54)
        (name "RXD0")
        (number "36")
      )
      (pin unspecified line
        (at 22.86 6.35 180)
        (length 2.54)
        (name "TXD0")
        (number "37")
      )
      (pin unspecified line
        (at 22.86 8.89 180)
        (length 2.54)
        (name "IO2")
        (number "38")
      )
      (pin unspecified line
        (at 22.86 11.43 180)
        (length 2.54)
        (name "IO1")
        (number "39")
      )
      (pin unspecified line
        (at 22.86 13.97 180)
        (length 2.54)
        (name "GND")
        (number "40")
      )
      (pin unspecified line
        (at 22.86 -24.13 180)
        (length 2.54)
        (name "EP")
        (number "41")
      )
    )
  )
)