(kicad_symbol_lib
  (version 20211014)
  (generator FastEDA)
  (symbol "ESP32-WROOM-32D"
    (in_bom yes)
    (on_board yes)
    (property
      "Reference"
      "U"
      (id 0)
      (at 0 29.21 0)
    )
    (property
      "Value"
      "ESP32-WROOM-32D"
      (id 1)
      (at 0 -29.21 0)
    )
    (property
      "Footprint"
      "ESP32-WROOM-32D-N8:WIFIM-SMD_39P-L25.5-W18.0-P1.27"
      (id 2)
      (at 0 -31.75 0)
    )
    (property
      "Datasheet"
      "https://lcsc.com/product-detail/WIFI-Modules_Espressif-Systems-ESP32-WROOM-32D-8MB_C529577.html"
      (id 3)
      (at 0 -34.29 0)
    )
    (property
      "Manufacturer"
      "ESPRESSIF(乐鑫)"
      (id 4)
      (at 0 -36.83 0)
    )
    (property
      "MPN"
      "ESP32-WROOM-32D-N8"
      (id 5)
      (at 0 -39.37 0)
    )
    (property
      "LCSC Part"
      "C529577"
      (id 6)
      (at 0 -41.91 0)
    )
    (property
      "ki_keywords"
      "WiFi Modules"
      (id 8)
      (at 0 -44.45 0)
    )
    (symbol "ESP32-WROOM-32D_0_1"
      (pin unspecified line
        (at 15.24 24.13 180)
        (length 2.54)
        (name "GND")
        (number "39")
      )
      (pin unspecified line
        (at 15.24 21.59 180)
        (length 2.54)
        (name "GND")
        (number "38")
      )
      (pin unspecified line
        (at 15.24 19.05 180)
        (length 2.54)
        (name "IO23")
        (number "37")
      )
      (pin unspecified line
        (at 15.24 16.51 180)
        (length 2.54)
        (name "IO22")
        (number "36")
      )
      (pin unspecified line
        (at 15.24 13.97 180)
        (length 2.54)
        (name "TXD0")
        (number "35")
      )
      (pin unspecified line
        (at 15.24 11.43 180)
        (length 2.54)
        (name "RXD0")
        (number "34")
      )
      (pin unspecified line
        (at 15.24 8.89 180)
        (length 2.54)
        (name "IO21")
        (number "33")
      )
      (pin unspecified line
        (at 15.24 6.35 180)
        (length 2.54)
        (name "NC")
        (number "32")
      )
      (pin unspecified line
        (at 15.24 3.81 180)
        (length 2.54)
        (name "IO19")
        (number "31")
      )
      (pin unspecified line
        (at 15.24 1.27 180)
        (length 2.54)
        (name "IO18")
        (number "30")
      )
      (pin unspecified line
        (at 15.24 -1.27 180)
        (length 2.54)
        (name "IO5")
        (number "29")
      )
      (pin unspecified line
        (at 15.24 -3.81 180)
        (length 2.54)
        (name "IO17")
        (number "28")
      )
      (pin unspecified line
        (at 15.24 -6.35 180)
        (length 2.54)
        (name "IO16")
        (number "27")
      )
      (pin unspecified line
        (at 15.24 -8.89 180)
        (length 2.54)
        (name "IO4")
        (number "26")
      )
      (pin unspecified line
        (at 15.24 -11.43 180)
        (length 2.54)
        (name "IO0")
        (number "25")
      )
      (pin unspecified line
        (at 15.24 -13.97 180)
        (length 2.54)
        (name "IO2")
        (number "24")
      )
      (pin unspecified line
        (at 15.24 -16.51 180)
        (length 2.54)
        (name "IO15")
        (number "23")
      )
      (pin unspecified line
        (at 15.24 -19.05 180)
        (length 2.54)
        (name "SD1")
        (number "22")
      )
      (pin unspecified line
        (at 15.24 -21.59 180)
        (length 2.54)
        (name "SD0")
        (number "21")
      )
      (pin unspecified line
        (at 15.24 -24.13 180)
        (length 2.54)
        (name "CLK")
        (number "20")
      )
      (pin unspecified line
        (at -15.24 -24.13 0)
        (length 2.54)
        (name "CMD")
        (number "19")
      )
      (pin unspecified line
        (at -15.24 -21.59 0)
        (length 2.54)
        (name "SD3")
        (number "18")
      )
      (pin unspecified line
        (at -15.24 -19.05 0)
        (length 2.54)
        (name "SD2")
        (number "17")
      )
      (pin unspecified line
        (at -15.24 -16.51 0)
        (length 2.54)
        (name "IO13")
        (number "16")
      )
      (pin unspecified line
        (at -15.24 -13.97 0)
        (length 2.54)
        (name "GND")
        (number "15")
      )
      (pin unspecified line
        (at -15.24 -11.43 0)
        (length 2.54)
        (name "IO12")
        (number "14")
      )
      (pin unspecified line
        (at -15.24 -8.89 0)
        (length 2.54)
        (name "IO14")
        (number "13")
      )
      (pin unspecified line
        (at -15.24 -6.35 0)
        (length 2.54)
        (name "IO27")
        (number "12")
      )
      (pin unspecified line
        (at -15.24 -3.81 0)
        (length 2.54)
        (name "IO26")
        (number "11")
      )
      (pin unspecified line
        (at -15.24 -1.27 0)
        (length 2.54)
        (name "IO25")
        (number "10")
      )
      (pin unspecified line
        (at -15.24 1.27 0)
        (length 2.54)
        (name "IO33")
        (number "9")
      )
      (pin unspecified line
        (at -15.24 3.81 0)
        (length 2.54)
        (name "IO32")
        (number "8")
      )
      (pin unspecified line
        (at -15.24 6.35 0)
        (length 2.54)
        (name "IO35")
        (number "7")
      )
      (pin unspecified line
        (at -15.24 8.89 0)
        (length 2.54)
        (name "IO34")
        (number "6")
      )
      (pin unspecified line
        (at -15.24 11.43 0)
        (length 2.54)
        (name "SENSOR_VN")
        (number "5")
      )
      (pin unspecified line
        (at -15.24 13.97 0)
        (length 2.54)
        (name "SENSOR_VP")
        (number "4")
      )
      (pin unspecified line
        (at -15.24 16.51 0)
        (length 2.54)
        (name "EN")
        (number "3")
      )
      (pin unspecified line
        (at -15.24 19.05 0)
        (length 2.54)
        (name "VDD33")
        (number "2")
      )
      (pin unspecified line
        (at -15.24 21.59 0)
        (length 2.54)
        (name "GND")
        (number "1")
      )
    )
  )
)