(kicad_symbol_lib
  (version 20211014)
  (generator FastEDA)
  (symbol "STM32F103ZET6"
    (in_bom yes)
    (on_board yes)
    (property
      "Reference"
      "U"
      (id 0)
      (at 0 95.25 0)
    )
    (property
      "Value"
      "STM32F103ZET6"
      (id 1)
      (at 0 -95.25 0)
    )
    (property
      "Footprint"
      "STM32F103ZET6:LQFP-144_L20.0-W20.0-P0.50-LS22.0-BL"
      (id 2)
      (at 0 -97.79 0)
    )
    (property
      "Datasheet"
      "https://lcsc.com/product-detail/ST-Microelectronics_STMicroelectronics_STM32F103ZET6_STM32F103ZET6_C8287.html"
      (id 3)
      (at 0 -100.33 0)
    )
    (property
      "Manufacturer"
      "ST(意法半导体)"
      (id 4)
      (at 0 -102.87 0)
    )
    (property
      "MPN"
      "STM32F103ZET6"
      (id 5)
      (at 0 -105.41 0)
    )
    (property
      "LCSC Part"
      "C8287"
      (id 6)
      (at 0 -107.95 0)
    )
    (property
      "ki_keywords"
      "ST Microelectronics"
      (id 8)
      (at 0 -110.49 0)
    )
    (property
      "ki_description"
      "ARM Cortex-M3 32-bit MCU, 512 KB Flash, 64 KB Internal RAM, 112 IOs, 144-pin LQFP, -40 to 85 degC, Tray"
      (id 9)
      (at 0 -113.03 0)
    )
    (symbol "STM32F103ZET6_0_1"
      (pin unspecified line
        (at -24.13 90.17 0)
        (length 2.54)
        (name "PE2")
        (number "1")
      )
      (pin unspecified line
        (at -24.13 87.63 0)
        (length 2.54)
        (name "PE3")
        (number "2")
      )
      (pin unspecified line
        (at -24.13 85.09 0)
        (length 2.54)
        (name "PE4")
        (number "3")
      )
      (pin unspecified line
        (at -24.13 82.55 0)
        (length 2.54)
        (name "PE5")
        (number "4")
      )
      (pin unspecified line
        (at -24.13 80.01 0)
        (length 2.54)
        (name "PE6")
        (number "5")
      )
      (pin unspecified line
        (at -24.13 77.47 0)
        (length 2.54)
        (name "VBAT")
        (number "6")
      )
      (pin unspecified line
        (at -24.13 74.93 0)
        (length 2.54)
        (name "PC13-TAMPER-RTC")
        (number "7")
      )
      (pin unspecified line
        (at -24.13 72.39 0)
        (length 2.54)
        (name "PC14-OSC32_IN")
        (number "8")
      )
      (pin unspecified line
        (at -24.13 69.85 0)
        (length 2.54)
        (name "PC15-OSC32_OUT")
        (number "9")
      )
      (pin unspecified line
        (at -24.13 67.31 0)
        (length 2.54)
        (name "PF0")
        (number "10")
      )
      (pin unspecified line
        (at -24.13 64.77 0)
        (length 2.54)
        (name "PF1")
        (number "11")
      )
      (pin unspecified line
        (at -24.13 62.23 0)
        (length 2.54)
        (name "PF2")
        (number "12")
      )
      (pin unspecified line
        (at -24.13 59.69 0)
        (length 2.54)
        (name "PF3")
        (number "13")
      )
      (pin unspecified line
        (at -24.13 57.15 0)
        (length 2.54)
        (name "PF4")
        (number "14")
      )
      (pin unspecified line
        (at -24.13 54.61 0)
        (length 2.54)
        (name "PF5")
        (number "15")
      )
      (pin unspecified line
        (at -24.13 52.07 0)
        (length 2.54)
        (name "VSS_5")
        (number "16")
      )
      (pin unspecified line
        (at -24.13 49.53 0)
        (length 2.54)
        (name "VDD_5")
        (number "17")
      )
      (pin unspecified line
        (at -24.13 46.99 0)
        (length 2.54)
        (name "PF6")
        (number "18")
      )
      (pin unspecified line
        (at -24.13 44.45 0)
        (length 2.54)
        (name "PF7")
        (number "19")
      )
      (pin unspecified line
        (at -24.13 41.91 0)
        (length 2.54)
        (name "PF8")
        (number "20")
      )
      (pin unspecified line
        (at -24.13 39.37 0)
        (length 2.54)
        (name "PF9")
        (number "21")
      )
      (pin unspecified line
        (at -24.13 36.83 0)
        (length 2.54)
        (name "PF10")
        (number "22")
      )
      (pin unspecified line
        (at -24.13 34.29 0)
        (length 2.54)
        (name "OSC_IN")
        (number "23")
      )
      (pin unspecified line
        (at -24.13 31.75 0)
        (length 2.54)
        (name "OSC_OUT")
        (number "24")
      )
      (pin unspecified line
        (at -24.13 29.21 0)
        (length 2.54)
        (name "NRST")
        (number "25")
      )
      (pin unspecified line
        (at -24.13 26.67 0)
        (length 2.54)
        (name "PC0")
        (number "26")
      )
      (pin unspecified line
        (at -24.13 24.13 0)
        (length 2.54)
        (name "PC1")
        (number "27")
      )
      (pin unspecified line
        (at -24.13 21.59 0)
        (length 2.54)
        (name "PC2")
        (number "28")
      )
      (pin unspecified line
        (at -24.13 19.05 0)
        (length 2.54)
        (name "PC3")
        (number "29")
      )
      (pin unspecified line
        (at -24.13 16.51 0)
        (length 2.54)
        (name "VSSA")
        (number "30")
      )
      (pin unspecified line
        (at -24.13 13.97 0)
        (length 2.54)
        (name "VREF-")
        (number "31")
      )
      (pin unspecified line
        (at -24.13 11.43 0)
        (length 2.54)
        (name "VREF+")
        (number "32")
      )
      (pin unspecified line
        (at -24.13 8.89 0)
        (length 2.54)
        (name "VDDA")
        (number "33")
      )
      (pin unspecified line
        (at -24.13 6.35 0)
        (length 2.54)
        (name "PA0-WKUP")
        (number "34")
      )
      (pin unspecified line
        (at -24.13 3.81 0)
        (length 2.54)
        (name "PA1")
        (number "35")
      )
      (pin unspecified line
        (at -24.13 1.27 0)
        (length 2.54)
        (name "PA2")
        (number "36")
      )
      (pin unspecified line
        (at -24.13 -1.27 0)
        (length 2.54)
        (name "PA3")
        (number "37")
      )
      (pin unspecified line
        (at -24.13 -3.81 0)
        (length 2.54)
        (name "VSS_4")
        (number "38")
      )
      (pin unspecified line
        (at -24.13 -6.35 0)
        (length 2.54)
        (name "VDD_4")
        (number "39")
      )
      (pin unspecified line
        (at -24.13 -8.89 0)
        (length 2.54)
        (name "PA4")
        (number "40")
      )
      (pin unspecified line
        (at -24.13 -11.43 0)
        (length 2.54)
        (name "PA5")
        (number "41")
      )
      (pin unspecified line
        (at -24.13 -13.97 0)
        (length 2.54)
        (name "PA6")
        (number "42")
      )
      (pin unspecified line
        (at -24.13 -16.51 0)
        (length 2.54)
        (name "PA7")
        (number "43")
      )
      (pin unspecified line
        (at -24.13 -19.05 0)
        (length 2.54)
        (name "PC4")
        (number "44")
      )
      (pin unspecified line
        (at -24.13 -21.59 0)
        (length 2.54)
        (name "PC5")
        (number "45")
      )
      (pin unspecified line
        (at -24.13 -24.13 0)
        (length 2.54)
        (name "PB0")
        (number "46")
      )
      (pin unspecified line
        (at -24.13 -26.67 0)
        (length 2.54)
        (name "PB1")
        (number "47")
      )
      (pin unspecified line
        (at -24.13 -29.21 0)
        (length 2.54)
        (name "PB2")
        (number "48")
      )
      (pin unspecified line
        (at -24.13 -31.75 0)
        (length 2.54)
        (name "PF11")
        (number "49")
      )
      (pin unspecified line
        (at -24.13 -34.29 0)
        (length 2.54)
        (name "PF12")
        (number "50")
      )
      (pin unspecified line
        (at -24.13 -36.83 0)
        (length 2.54)
        (name "VSS_6")
        (number "51")
      )
      (pin unspecified line
        (at -24.13 -39.37 0)
        (length 2.54)
        (name "VDD_6")
        (number "52")
      )
      (pin unspecified line
        (at -24.13 -41.91 0)
        (length 2.54)
        (name "PF13")
        (number "53")
      )
      (pin unspecified line
        (at -24.13 -44.45 0)
        (length 2.54)
        (name "PF14")
        (number "54")
      )
      (pin unspecified line
        (at -24.13 -46.99 0)
        (length 2.54)
        (name "PF15")
        (number "55")
      )
      (pin unspecified line
        (at -24.13 -49.53 0)
        (length 2.54)
        (name "PG0")
        (number "56")
      )
      (pin unspecified line
        (at -24.13 -52.07 0)
        (length 2.54)
        (name "PG1")
        (number "57")
      )
      (pin unspecified line
        (at -24.13 -54.61 0)
        (length 2.54)
        (name "PE7")
        (number "58")
      )
      (pin unspecified line
        (at -24.13 -57.15 0)
        (length 2.54)
        (name "PE8")
        (number "59")
      )
      (pin unspecified line
        (at -24.13 -59.69 0)
        (length 2.54)
        (name "PE9")
        (number "60")
      )
      (pin unspecified line
        (at -24.13 -62.23 0)
        (length 2.54)
        (name "VSS_7")
        (number "61")
      )
      (pin unspecified line
        (at -24.13 -64.77 0)
        (length 2.54)
        (name "VDD_7")
        (number "62")
      )
      (pin unspecified line
        (at -24.13 -67.31 0)
        (length 2.54)
        (name "PE10")
        (number "63")
      )
      (pin unspecified line
        (at -24.13 -69.85 0)
        (length 2.54)
        (name "PE11")
        (number "64")
      )
      (pin unspecified line
        (at -24.13 -72.39 0)
        (length 2.54)
        (name "PE12")
        (number "65")
      )
      (pin unspecified line
        (at -24.13 -74.93 0)
        (length 2.54)
        (name "PE13")
        (number "66")
      )
      (pin unspecified line
        (at -24.13 -77.47 0)
        (length 2.54)
        (name "PE14")
        (number "67")
      )
      (pin unspecified line
        (at -24.13 -80.01 0)
        (length 2.54)
        (name "PE15")
        (number "68")
      )
      (pin unspecified line
        (at -24.13 -82.55 0)
        (length 2.54)
        (name "PB10")
        (number "69")
      )
      (pin unspecified line
        (at -24.13 -85.09 0)
        (length 2.54)
        (name "PB11")
        (number "70")
      )
      (pin unspecified line
        (at -24.13 -87.63 0)
        (length 2.54)
        (name "VSS_1")
        (number "71")
      )
      (pin unspecified line
        (at -24.13 -90.17 0)
        (length 2.54)
        (name "VDD_1")
        (number "72")
      )
      (pin unspecified line
        (at 21.59 -90.17 180)
        (length 2.54)
        (name "PB12")
        (number "73")
      )
      (pin unspecified line
        (at 21.59 -87.63 180)
        (length 2.54)
        (name "PB13")
        (number "74")
      )
      (pin unspecified line
        (at 21.59 -85.09 180)
        (length 2.54)
        (name "PB14")
        (number "75")
      )
      (pin unspecified line
        (at 21.59 -82.55 180)
        (length 2.54)
        (name "PB15")
        (number "76")
      )
      (pin unspecified line
        (at 21.59 -80.01 180)
        (length 2.54)
        (name "PD8")
        (number "77")
      )
      (pin unspecified line
        (at 21.59 -77.47 180)
        (length 2.54)
        (name "PD9")
        (number "78")
      )
      (pin unspecified line
        (at 21.59 -74.93 180)
        (length 2.54)
        (name "PD10")
        (number "79")
      )
      (pin unspecified line
        (at 21.59 -72.39 180)
        (length 2.54)
        (name "PD11")
        (number "80")
      )
      (pin unspecified line
        (at 21.59 -69.85 180)
        (length 2.54)
        (name "PD12")
        (number "81")
      )
      (pin unspecified line
        (at 21.59 -67.31 180)
        (length 2.54)
        (name "PD13")
        (number "82")
      )
      (pin unspecified line
        (at 21.59 -64.77 180)
        (length 2.54)
        (name "VSS_8")
        (number "83")
      )
      (pin unspecified line
        (at 21.59 -62.23 180)
        (length 2.54)
        (name "VDD_8")
        (number "84")
      )
      (pin unspecified line
        (at 21.59 -59.69 180)
        (length 2.54)
        (name "PD14")
        (number "85")
      )
      (pin unspecified line
        (at 21.59 -57.15 180)
        (length 2.54)
        (name "PD15")
        (number "86")
      )
      (pin unspecified line
        (at 21.59 -54.61 180)
        (length 2.54)
        (name "PG2")
        (number "87")
      )
      (pin unspecified line
        (at 21.59 -52.07 180)
        (length 2.54)
        (name "PG3")
        (number "88")
      )
      (pin unspecified line
        (at 21.59 -49.53 180)
        (length 2.54)
        (name "PG4")
        (number "89")
      )
      (pin unspecified line
        (at 21.59 -46.99 180)
        (length 2.54)
        (name "PG5")
        (number "90")
      )
      (pin unspecified line
        (at 21.59 -44.45 180)
        (length 2.54)
        (name "PG6")
        (number "91")
      )
      (pin unspecified line
        (at 21.59 -41.91 180)
        (length 2.54)
        (name "PG7")
        (number "92")
      )
      (pin unspecified line
        (at 21.59 -39.37 180)
        (length 2.54)
        (name "PG8")
        (number "93")
      )
      (pin unspecified line
        (at 21.59 -36.83 180)
        (length 2.54)
        (name "VSS_9")
        (number "94")
      )
      (pin unspecified line
        (at 21.59 -34.29 180)
        (length 2.54)
        (name "VDD_9")
        (number "95")
      )
      (pin unspecified line
        (at 21.59 -31.75 180)
        (length 2.54)
        (name "PC6")
        (number "96")
      )
      (pin unspecified line
        (at 21.59 -29.21 180)
        (length 2.54)
        (name "PC7")
        (number "97")
      )
      (pin unspecified line
        (at 21.59 -26.67 180)
        (length 2.54)
        (name "PC8")
        (number "98")
      )
      (pin unspecified line
        (at 21.59 -24.13 180)
        (length 2.54)
        (name "PC9")
        (number "99")
      )
      (pin unspecified line
        (at 21.59 -21.59 180)
        (length 2.54)
        (name "PA8")
        (number "100")
      )
      (pin unspecified line
        (at 21.59 -19.05 180)
        (length 2.54)
        (name "PA9")
        (number "101")
      )
      (pin unspecified line
        (at 21.59 -16.51 180)
        (length 2.54)
        (name "PA10")
        (number "102")
      )
      (pin unspecified line
        (at 21.59 -13.97 180)
        (length 2.54)
        (name "PA11")
        (number "103")
      )
      (pin unspecified line
        (at 21.59 -11.43 180)
        (length 2.54)
        (name "PA12")
        (number "104")
      )
      (pin unspecified line
        (at 21.59 -8.89 180)
        (length 2.54)
        (name "PA13")
        (number "105")
      )
      (pin unspecified line
        (at 21.59 -6.35 180)
        (length 2.54)
        (name "NC")
        (number "106")
      )
      (pin unspecified line
        (at 21.59 -3.81 180)
        (length 2.54)
        (name "VSS_2")
        (number "107")
      )
      (pin unspecified line
        (at 21.59 -1.27 180)
        (length 2.54)
        (name "VDD_2")
        (number "108")
      )
      (pin unspecified line
        (at 21.59 1.27 180)
        (length 2.54)
        (name "PA14")
        (number "109")
      )
      (pin unspecified line
        (at 21.59 3.81 180)
        (length 2.54)
        (name "PA15")
        (number "110")
      )
      (pin unspecified line
        (at 21.59 6.35 180)
        (length 2.54)
        (name "PC10")
        (number "111")
      )
      (pin unspecified line
        (at 21.59 8.89 180)
        (length 2.54)
        (name "PC11")
        (number "112")
      )
      (pin unspecified line
        (at 21.59 11.43 180)
        (length 2.54)
        (name "PC12")
        (number "113")
      )
      (pin unspecified line
        (at 21.59 13.97 180)
        (length 2.54)
        (name "PD0")
        (number "114")
      )
      (pin unspecified line
        (at 21.59 16.51 180)
        (length 2.54)
        (name "PD1")
        (number "115")
      )
      (pin unspecified line
        (at 21.59 19.05 180)
        (length 2.54)
        (name "PD2")
        (number "116")
      )
      (pin unspecified line
        (at 21.59 21.59 180)
        (length 2.54)
        (name "PD3")
        (number "117")
      )
      (pin unspecified line
        (at 21.59 24.13 180)
        (length 2.54)
        (name "PD4")
        (number "118")
      )
      (pin unspecified line
        (at 21.59 26.67 180)
        (length 2.54)
        (name "PD5")
        (number "119")
      )
      (pin unspecified line
        (at 21.59 29.21 180)
        (length 2.54)
        (name "VSS_10")
        (number "120")
      )
      (pin unspecified line
        (at 21.59 31.75 180)
        (length 2.54)
        (name "VDD_10")
        (number "121")
      )
      (pin unspecified line
        (at 21.59 34.29 180)
        (length 2.54)
        (name "PD6")
        (number "122")
      )
      (pin unspecified line
        (at 21.59 36.83 180)
        (length 2.54)
        (name "PD7")
        (number "123")
      )
      (pin unspecified line
        (at 21.59 39.37 180)
        (length 2.54)
        (name "PG9")
        (number "124")
      )
      (pin unspecified line
        (at 21.59 41.91 180)
        (length 2.54)
        (name "PG10")
        (number "125")
      )
      (pin unspecified line
        (at 21.59 44.45 180)
        (length 2.54)
        (name "PG11")
        (number "126")
      )
      (pin unspecified line
        (at 21.59 46.99 180)
        (length 2.54)
        (name "PG12")
        (number "127")
      )
      (pin unspecified line
        (at 21.59 49.53 180)
        (length 2.54)
        (name "PG13")
        (number "128")
      )
      (pin unspecified line
        (at 21.59 52.07 180)
        (length 2.54)
        (name "PG14")
        (number "129")
      )
      (pin unspecified line
        (at 21.59 54.61 180)
        (length 2.54)
        (name "VSS_11")
        (number "130")
      )
      (pin unspecified line
        (at 21.59 57.15 180)
        (length 2.54)
        (name "VDD_11")
        (number "131")
      )
      (pin unspecified line
        (at 21.59 59.69 180)
        (length 2.54)
        (name "PG15")
        (number "132")
      )
      (pin unspecified line
        (at 21.59 62.23 180)
        (length 2.54)
        (name "PB3")
        (number "133")
      )
      (pin unspecified line
        (at 21.59 64.77 180)
        (length 2.54)
        (name "PB4")
        (number "134")
      )
      (pin unspecified line
        (at 21.59 67.31 180)
        (length 2.54)
        (name "PB5")
        (number "135")
      )
      (pin unspecified line
        (at 21.59 69.85 180)
        (length 2.54)
        (name "PB6")
        (number "136")
      )
      (pin unspecified line
        (at 21.59 72.39 180)
        (length 2.54)
        (name "PB7")
        (number "137")
      )
      (pin unspecified line
        (at 21.59 74.93 180)
        (length 2.54)
        (name "BOOT0")
        (number "138")
      )
      (pin unspecified line
        (at 21.59 77.47 180)
        (length 2.54)
        (name "PB8")
        (number "139")
      )
      (pin unspecified line
        (at 21.59 80.01 180)
        (length 2.54)
        (name "PB9")
        (number "140")
      )
      (pin unspecified line
        (at 21.59 82.55 180)
        (length 2.54)
        (name "PE0")
        (number "141")
      )
      (pin unspecified line
        (at 21.59 85.09 180)
        (length 2.54)
        (name "PE1")
        (number "142")
      )
      (pin unspecified line
        (at 21.59 87.63 180)
        (length 2.54)
        (name "VSS_3")
        (number "143")
      )
      (pin unspecified line
        (at 21.59 90.17 180)
        (length 2.54)
        (name "VDD_3")
        (number "144")
      )
    )
  )
)